STEAM POWER SYSTEM
1. Why Thermal Power Plants are always situated by the side of rivers or lakes?
2. Why cooling towers require in the Steam power plant 
3. What is the overall efficiency of the Thermal Power Plant or Steam Power Plant
4. What is the Thermal efficiency of steam power plant
5. Steam power plant works on which cycle
6. Why are feed water heaters are used
7. What is the effect of increasing steam pressure on efficiency of steam power plant
8. What is the effect of increasing steam temperature of thermal power plant on its thermal efficiency
9. What could be the impacts of Air Pollution on Vegetation
  (a)    high CO content in flue gases at exit
  (b)    high CO2 content in flue gases at exit
  (c)    high temperature of flue gases
  (d)    the smoking exhaust from chimney
         10 Solar thermal power generation can be achieved by
  (a)    using focusing collector or heliostates
  (b)    using flat plate collectors
  (c)    using a solar pond
  (d)    any of the above system
         11  A steam power station requires space
           (a)    equal to diesel power station
           (b)    more than diesel power station
           (c)    less than diesel power station
         12   The draught produced, for a given height of the chimney and  given    Mean temperature of chimney gases
   (a)    decreases with increase in outside air temperature
   (b)    increases with increase in outside air temperature
   (c)    remains the same irrespective of outside air temperature
    (d)    may increase or decrease with increase in outside air temperature
        13The draught in locomotive boilers is produced by
    (a)     forced fan
    (b)     chimney
    (c)     steam jet
    (d)     only motion of locomotive
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14.       Artificial draught is produced by
     (a)     air fans
     (b)     steam jet
     (c)     fan or steam jet
     (d)     all of the above
15.    The artificial draught normally is designed to produce
     (a)     less smoke
     (b)     more draught
     (c)     less chimney gas temperature
     (d)     all of the above
16.     In India largest thermal power station is located at
               (a)    Kota
               (b)    Sarni
               (c)    Chandrapur
               (d)    Neyveli
17.     Artificial draught is produced by
                (a)     induced fan
                (b)     forced fan
                (c)     induced and forced fan
                (d)     all of the above





